{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["高清监控系统"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"高清监控系统","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"merged":[[0,0,0,7],[2,0,2,6],[11,0,11,6],[17,0,17,6],[23,2,23,7]],"flags":["formulas_cached_only"]}
["娄底职院宿舍楼高清监控系统清单"]
["序号","名称","参数","单位","数量","单价（元）","金额（元）","备注"]
["一、前端设备 "]
[1,"网络监控摄像机","400万星光级(室外)\n1/2.7”CMOS ICR红外阵列筒型网络摄像机;\n最小照度 0.005Lux @(F1.2,AGC ON) ,0 Lux with IR\n快门 1/3秒至1/100,000秒\n慢快门 支持\n镜头 4mm, 水平视场角79°(6mm,8mm,12mm可选)\n镜头接口类型 M12\n日夜转换模式 ICR红外滤片式\n数字降噪 3D数字降噪\n宽动态范围 120dB\n视频压缩标准 H.265 /H.264/ MJPEG\n帧率 50Hz: 25fps (2560× 1920,2560× 1536,1920 × 1080 ,1280 × 720) \n感兴趣区域ROI支持三码流分别设置1个固定区域\n行为分析 越界侦测,区域入侵侦测,进入/离开区域侦测,徘徊侦测,人员聚集侦测,快速运动侦测,停车侦测,物品遗留/拿取侦测\n异常侦测 场景变更侦测，虚焦侦测\n识别检测 支持人脸侦测\n通讯接口 1个RJ45 10M / 100M 自适应以太网口\n工作温度和湿度 -30℃~60℃,湿度小于95%(无凝结)\n电源供应 DC12V±25% / PoE(802.3af)；\nPoE：8W Max\n红外照射距离最远可达50米\n防护等级 IP67","台",6]
[2,"网络监控摄像机","400万星光级(室内)\n1/2.7\" CMOS 全彩筒型网络摄像机 ;\n最小照度 0.0002Lux @(F1.2,AGC ON) ,0 Lux with IR\n快门 1/3秒至1/100,000秒\n慢快门 支持\n镜头 4mm, 水平视场角79°(6mm,8mm,12mm可选)\n镜头接口类型 M12\n日夜转换模式 ICR红外滤片式\n数字降噪 3D数字降噪\n宽动态范围 120dB\n视频压缩标准 H.265 /H.264/ MJPEG\n帧率 50Hz: 25fps (1920 × 1080 ,1280 × 720) \n感兴趣区域ROI支持三码流分别设置1个固定区域\n行为分析 越界侦测,区域入侵侦测,进入/离开区域侦测,徘徊侦测,人员聚集侦测,快速运动侦测,停车侦测,物品遗留/拿取侦测\n异常侦测 场景变更侦测，虚焦侦测\n识别检测 支持人脸侦测\n通讯接口 1个RJ45 10M / 100M 自适应以太网口\n工作温度和湿度 -30℃~60℃,湿度小于95%(无凝结)\n电源供应 DC12V±25% / PoE(802.3af)；\nPoE：5.5W Max\n红外照射距离 最远可达30米\n防护等级 IP67","台",31,{"v":510,"d":"510.00"},{"v":15810,"d":"15,810.00"}]
[3,"接入交换机","24个10/100/1000Base-TX电口+4千兆SFP(光) POE交换机","台",2]
[4,"墙柜","6U墙柜","台",3]
[5,"摄像机支架","支架","个",37]
[6,"宿管室","视频解码器","台",1]
[7,null,"显示屏24寸","台",1]
[8,null,"鼠标键盘等配件","套",1]
["二、机房设备 "]
[1,"网络存储设备","16盘位控制器磁盘阵列；256Mbps接入带宽,2个千兆网口(不可扩展)；3U机架式单控制器、冗余电源、支持SATA硬盘；64位多核处理器、4GB缓存（可扩展至8G）；不支持扩展柜\nRAID级别：RAID0、1、5、JBOD、Hot-Spare;数据保护：系统信息实时备份、卷克隆;\n不支持且不可定制SANNAS功能","台",1]
[2,"企业级硬盘","HDD,ST6000NM021A,6TB,7200,3.5\",SATA","个",8]
[3,"平台软件增容","不支持且不可定制SANNAS功能","路",37,null,"不能计费","共用主机房平台"]
[4,"视频服务器","4114×1/16G DDR4×2/1TB 7.2K SATA×2/SAS_HBA/1GbE×2/550W(1+1)/2U/16DIMM\n2U双路标准机架式服务器\nCPU：1颗Xeon® Silver 4114（10核，2.2GHz）\n内存：16G*2 DDR4，16根内存插槽，最大支持扩展至1TB内存\n硬盘：2块1T 7.2K 3.5寸 SATA硬盘，最高可支持12块3.5寸（兼容2.5寸）热插拔SAS/SATA硬盘\n阵列卡：SAS_HBA卡，支持RAID 0/1/10\nPCIE扩展：最大可支持6个PCIE扩展插槽\n网口：2个千兆电口\n其他接口：1个RJ45管理接口，4个USB 3.0接口，2个VGA接口\n电源：标配550W（1+1）高效铂金CRPS冗余电源 \n机箱规格：87mm(高)x 447mm(宽)x720mm(深)\n设备重量：约33千克（含导轨）\n操作系统:HIK OS","台",1,null,"不能计费","共用主机房平台"]
[5,"光模块","单模光模块 SFP-GE","个",2]
["三、传输及辅助设备 "]
[1,"网线","0.57mm工程级蓝色，CAT6网线 305米/箱","箱",8]
[2,"PVC管","25MM","米",600]
[3,"电源线","RVV3*1.5","米",600]
[4,"光纤","12芯单模，铠装室外光纤","米",600]
[5,"其他"," 辅材","批",1]
[null,"总计费用","本项目总计费用为人民币壹拾壹万元整（￥110000.00），包含所有费用。平台软件增容、视频服务器共用学校原有主机房平台。"]